**communication iOT / nodes Server**

* AT

OK

* AT+CWJAP=“SSID”,”Password"
* (- AT+CWJAP=“routeur”,”routeurbjtu")

Query AT+CWJAP? +CWJAP:"RochefortSurLac" OK

* AT+CIFSR

AT+CIFSR 192.168.0.105

OK

**2 STATES**

**—> POST DATA to the server**

**—> Listen commands**